For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear Floor Console Rear Trim Upper Panel Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Rear Floor Console Rear Trim Upper Panel Screw (Qty: 2) Tighten 2.5 N·m (22 lb in)
3 | Rear Floor Console Rear Trim Upper Panel Assembly

#### Procedure

Use a flat-bladed plastic trim tool in order to release the clips securing the trim panel to the console assembly.