For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the headlining trim panel. Refer to Headlining Trim Panel Replacement.

1 | Sunroof Module Bolt (Qty: 12) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Sunroof Module Assembly Note: A new sunroof module assembly does not include the sunroof window, the motor, the sunshade, or the finishing lace as components. You must install the old components to the new sunroof module assembly.