For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Warning in the Preface section.

#### Preliminary Procedure

1. Disable the SIR system. Refer to SIR Disabling and Enabling.
2. Remove the instrument panel assembly. Refer to Instrument Panel Assembly Replacement.

1 | Instrument Panel Inflatable Restraint Module Nut (Qty: 7) Caution: Refer to Fastener Caution in the Preface section. Tighten 8 N·m (71 lb in)
2 | Instrument Panel Inflatable Restraint Module Assembly Tip Disconnect the electrical connectors.