For 1990-2009 cars

#### Special Tools

EN 49424 Remover and Installer Ignition Module

For equivalent regional tools, refer to Special Tools.

Note: Note the arrow on the cover.

1. Remove the cover of the DIS ignition coil in the direction of the arrow.
2. Remove the 2 ignition coil bolts.
3. Install the EN 49424 remover/installer (1).
4. Remove the ignition coil module (2) with the EN 49424 remover/installer (1).