For 1990-2009 cars

## Engine Coolant Temperature Sensor Replacement Radiator

Callout | Component Name
--- | ---

#### Preliminary Procedure

Drain the cooling system. Refer to Cooling System Draining and Filling.

1 | Engine Coolant Temperature Sensor Fastener

#### Procedure

Remove the engine coolant temperature sensor.

2 | Unlock the Retaining Clamp
3 | Disconnect the Wiring Harness Plug

## Engine Coolant Temperature Sensor Replacement Thermostat

Callout | Component Name
--- | ---

#### Preliminary Procedure

Drain the cooling system. Refer to Cooling System Draining and Filling.

1 | Engine Coolant Temperature Sensor Fastener

#### Procedure

Remove the engine coolant temperature sensor.

2 | Unlock the Retaining Clamp
3 | Disconnect the Wiring Harness Plug