For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
B0000 | Vehicle Speed Information Circuit | Radio | DTC B0000
B0012 | Driver Frontal Deployment Loop Stage 1 | SDM | DTC B0012 or B0013
B0013 | Driver Frontal Deployment Loop Stage 2 | SDM | DTC B0012 or B0013
B0014 | Driver Side Deployment Loop | SDM | DTC B0014-B0045
B0016 | Left Roof Rail Deployment Loop Stage 1 | SDM | DTC B0014-B0045
B0018 | Left Roof Rail Deployment Loop Stage 2 | SDM | DTC B0014-B0045
B0019 | Passenger Frontal Deployment Loop Stage 1 | SDM | DTC B0014-B0045
B001A | Driver Seat Belt Pretensioner Deployment Loop 2 | SDM | DTC B001A
B001B | Passenger Seat Belt Pretensioner Deployment Loop 2 | SDM | DTC B001B
B0020 | Passenger Frontal Deployment Loop Stage 2 | SDM | DTC B0014-B0045
B0021 | Passenger Side Deployment Loop | SDM | DTC B0014-B0045
B0023 | Right Roof Rail Deployment Loop Stage 1 | SDM | DTC B0014-B0045
B0025 | Right Roof Rail Deployment Loop Stage 2 | SDM | DTC B0014-B0045
B0051 | Deployment Commanded | SDM | DTC B0051
B0052 | Deployment Commanded | SDM | DTC B0052
B0072 | Left Front Seat Belt Sensor Circuit | SDM | DTC B0072
B0073 | Right Front Seat Belt Sensor Circuit | SDM | DTC B0073
B0081 | Passenger Presence Module | SDM | DTC B0081
B0083 | Front Impact Sensor 1 | SDM | DTC B0083-B0088
B0084 | Front Impact Sensor 2 | SDM | DTC B0083-B0088
B0085 | Left Front Side Impact Sensor | SDM | DTC B0083-B0088
B0086 | Right Front Side Impact Sensor | SDM | DTC B0083-B0088
B0087 | Left Rear Side Impact Sensor | SDM | DTC B0083-B0088
B0088 | Right Rear Side Impact Sensor | SDM | DTC B0083-B0088
B0158 | Outside Air Temperature Sensor Circuit | Instrument Cluster | DTC B0158
B0163 | Passenger Compartment Temperature Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0158
B0173 | Upper Outlet Air Temperature Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0173, B0178, or B3933
B0178 | Lower Left Outlet Air Temperature Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0173, B0178, or B3933
B0183 | Solar Load Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0158
B018A | Windshield Temperature Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B018A, B048C, B048F, or B1395
B0193 | Front Blower Motor Speed Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0193 for the automatic system or DTC B0193 for the manual system
B0223 | Recirculate Position Command 1 Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0223, B0233, B023A, or B0408 for the automatic system or DTC B0223, B0233, B023A, or B0408 for the manual system
B0233 | Air Flow Control Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0223, B0233, B023A, or B0408 for the automatic system or DTC B0223, B0233, B023A, or B0408 for the manual system
B023A | HVAC Actuators Supply Voltage | Heater and Blower and Air Conditioning Control Module | DTC B0223, B0233, B023A, or B0408 for the automatic system or DTC B0223, B0233, B023A, or B0408 for the manual system
B0283 | Rear Defrost Circuit | BCM | DTC B0283
B0408 | Main Temperature Control Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0223, B0233, B023A, or B0408 for the automatic system or DTC B0223, B0233, B023A, or B0408 for the manual system
B048C | Humidity Sensor Humidity Circuit | Heater and Blower and Air Conditioning Control Module | DTC B018A, B048C, B048F, or B1395
B040D | Auxiliary Heater Temperature Command Circuit | Heater and Blower and Air Conditioning Control Module | DTC B048D or B048E for the automatic system or DTC B048D or B048E for the manual system
B040E | Auxiliary Heater System Malfunction | Heater and Blower and Air Conditioning Control Module | DTC B048D or B048E for the automatic system or DTC B048D or B048E for the manual system
B048F | Humidity Sensor Temperature Circuit | Heater and Blower and Air Conditioning Control Module | DTC B018A, B048C, B048F, or B1395
B0550 | Odometer Circuit | Instrument Cluster | DTC B0550
B0685 | Security System Indicator Circuit | BCM | DTC B0685
B0958 | Parking Aid Rear Sensor Left Corner Circuit | Object Alarm Module | DTC B0958, B0959, B0960, or B0961
B0959 | Parking Aid Rear Sensor Left Middle Circuit | Object Alarm Module | DTC B0958, B0959, B0960, or B0961
B0960 | Parking Aid Rear Sensor Right Middle Circuit | Object Alarm Module | DTC B0958, B0959, B0960, or B0961
B0961 | Parking Aid Rear Sensor Right Corner Circuit | Object Alarm Module | DTC B0958, B0959, B0960, or B0961
B096A | Hazard Lamps Switch Backlighting Circuit | BCM | DTC B096A
B1001 | Option Configuration | BCM | DTC B1001
SDM | DTC B1001
B1015 | Vehicle Identification Number Information Error | Object Alarm Module | DTC B1015
B1019 | System Configuration Error | SDM | DTC B1019
B101D | ECU Hardware | SDM | DTC B101D
B101E | ECU Software | BCM | DTC B101E
SDM | DTC B101E
B1020 | Auxiliary Electronic Control Unit Performance | Radio | DTC B1020
B1023 | Integral Switch Performance | Steering Column Lock Control Module | DTC B1023
B1025 | Left Front Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1035 | Right Front Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1045 | Left Rear Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1055 | Right Rear Audio Output Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1259 | Antenna Ground Circuit | Digital Audio Broadcast Receiver | DTC B1259
B1271 | Theft Protection Active | Radio | DTC B1271
B1278 | Left Auxiliary Input Signal Circuit | Radio | DTC B1278 or B1279
B1279 | Right Auxiliary Input Signal Circuit | Radio | DTC B1278 or B1279
B1287 | Amplifier Control Signal Circuit | Radio | DTC B1287
B1325 | Control Module Power Circuit |  | DTC B1325
B1370 | Control Module Ignition On and Start Circuit | BCM | DTC B1370-B1379, B1380-B1389, or B1440-B1443
B1380 | Control Module Ignition Accessory Circuit | BCM | DTC B1370-B1379, B1380-B1389, or B1440-B1443
B138A | Control Module Voltage Reference Output Circuit | Object Alarm Module | DTC B138A
B1395 | Control Module Voltage Reference Output Circuit | Heater and Blower and Air Conditioning Control Module | DTC B018A, B048C, B048F, or B1395
B1405 | Control Module Voltage Reference Output 2 | BCM | DTC B1405
B1441 | Control Module Ignition Off, Run, and Start Circuit | BCM | DTC B1370-B1379, B1380-B1389, or B1440-B1443
B1445 | Control Module Voltage Output Circuit | BCM | DTC B1445
B144A | RUN Power Relay Circuit | BCM | DTC B144A
B1474 | Right Front Exterior Door Handle Switch Circuit | Keyless Entry Control Module | DTC B1474
B147E | Logistics Mode Relay Set Secondary Circuit | BCM | DTC B147E
B147F | Logistics Mode Relay Reset Secondary Circuit | BCM | DTC B147F
B1480 | Battery Rundown Protection Circuit | BCM |
B1516 | Battery Current Sensor | BCM | DTC B1516
B1517 | Battery Voltage | BCM | DTC B1517
B1527 | Parasitic Load | BCM | DTC B1527
B1529 | Control Module Voltage Reference Output 5 Circuit | BCM | DTC B1529
B1534 | Left Rear Door Handle Switch Circuit | Keyless Entry Control Module | DTC B1534 or B1535
B1535 | Right Rear Door Handle Switch Circuit | Keyless Entry Control Module | DTC B1534 or B1535
B1543 | Liftgate Exterior Lock Switch Circuit | Keyless Entry Control Module | DTC B1543
B1925 | Left Seat Cushion Heater Sensor Circuit | Heated Seat Module | DTC B1925 or B2170
B2170 | Right Seat Cushion Heater Sensor Circuit | Heated Seat Module | DTC B1925 or B2170
B2345 | Front Seat Heater Disable Circuit | Memory Seat Module |
B2425 | Left Seat Cushion Heater Circuit | Heated Seat Module | DTC B2425 or B2430
B242A | Seat Heaters Common Circuit | Heated Seat Module | DTC B242A
B2430 | Right Seat Cushion Heater Circuit | Heated Seat Module | DTC B2425 or B2430
B2462 | Global Positioning System Signal |  | DTC B2462
B2494 | Liftgate Handle Switch Circuit | Keyless Entry Control Module | DTC B2494
B250B | Left Front Door Unlatch Low Control Circuit | BCM | DTC B250B
B2515 | Steering Column Lock Motor Feedback Circuit | Steering Column Lock Control Module | DTC B2515
B2516 | Driver Exterior Lock Switch Circuit | BCM | DTC B2516
B251A | All Door Unlatch Circuit | BCM | DTC B251A or B251B
B251B | Driver Door Unlatch High Control Circuit | BCM | DTC B251A or B251B
B2530 | Front Fog Lamps Control Circuit | BCM | DTC B2530
B2540 | Rear Fog Lamps Control Circuit | BCM | DTC B2540
B2545 | Backup Lamps Control Circuit | BCM | DTC B2545
B2575 | Left Headlamp Control Circuit | Headlamp Control Module | DTC B2575 or B2699
B257A | Headlamp Switch Input Signals Correlation | BCM | DTC B257A
B257B | Lighting Control Switch Signal | BCM | DTC B257B
B2580 | High Beam Control Circuit | BCM | DTC B2580
B2585 | Park Lamps Control Circuit | BCM | DTC B2585 or B3867
B2610 | Passenger Compartment Dimming 1 Circuit | BCM | DTC B2610
B270A | Park Lock Solenoid Actuator Control Circuit | BCM | DTC B270A
B2740 | Front Fog Lamp Switch Circuit | BCM | DTC B2740
B2705 | Horn Relay Secondary Circuit | BCM | DTC B2750
B2897 | Steering Column Lock Motor Lock Circuit | Steering Column Lock Control Module | DTC B2897
B2910 | Steering Column Lock Password Incorrect | Steering Column Lock Control Module | DTC B2910
B291B | Content Theft Deterrent Sensor | BCM | DTC B291B
B3006 | Hood Ajar Circuit | BCM | DTC B3006
B3031 | Security Controller In Learn Mode | BCM | DTC B3031
B3055 | No Transponder Modulation or No Transponder | BCM | DTC B3055
B305A | No Response From Steering Column Lock Received | BCM | DTC B305A
B3060 | Unprogrammed Transponder Identification Code Received | BCM | DTC B3060
B3101 | Keyless Entry Data Link Circuit | BCM | DTC B3101
B3105 | Keyless Entry System Key Fobs | BCM | DTC B3105
B3106 | Keyless Entry Data Link | BCM | DTC B3106
B3109 | Keyless Transmitter 1 Battery | Remote Control Door Lock Receiver | DTC B3109-B3113
B310D | Keyless Entry Transmitter 6 Battery | Remote Control Door Lock Receiver | DTC B310D-B310F
B310E | Keyless Entry Transmitter 7 Battery | Remote Control Door Lock Receiver | DTC B310D-B310F
B310F | Keyless Entry Transmitter 8 Battery | Remote Control Door Lock Receiver | DTC B310D-B310F
B3110 | Keyless Entry Transmitter 2 Battery | Remote Control Door Lock Receiver | DTC B3109-B3113
B3111 | Keyless Entry Transmitter 3 Battery | Remote Control Door Lock Receiver | DTC B3109-B3113
B3112 | Keyless Entry Transmitter 4 Battery | Remote Control Door Lock Receiver | DTC B3109-B3113
B3113 | Keyless Entry Transmitter 5 Battery | Remote Control Door Lock Receiver | DTC B3109-B3113
B3119 | Keyless Entry Antenna 1 | Remote Control Door Lock Receiver | DTC B3119
B3120 | Keyless Entry Antenna 2 | Remote Control Door Lock Receiver | DTC B3120
B3121 | Keyless Entry Antenna 3 | Remote Control Door Lock Receiver | DTC B3121
B3122 | Keyless Entry Antenna 4 | Remote Control Door Lock Receiver | DTC B3122
B2123 | Keyless Entry Antenna 5 | Remote Control Door Lock Receiver | DTC B3123
B2124 | Keyless Entry Antenna 6 | Remote Control Door Lock Receiver | DTC B3124
B3125 | Driver Door Only Unlock Circuit | BCM | DTC B3125, B3130, or B3135
B3130 | All Door Unlock Circuit | BCM | DTC B3125, B3130, or B3135
B3135 | All Door Lock Circuit | BCM | DTC B3125, B3130, or B3135
B316B | Driver Window Switch | Driver Door Module, Passenger Door Module | DTC B316B, B317A, B318A, or B319A
B317A | Passenger Window Switch | Driver Door Module, Passenger Door Module | DTC B316B, B317A, B318A, or B319A
B318A | Left Rear Window Switch | Driver Door Module, Passenger Door Module | DTC B316B, B317A, B318A, or B319A
B319A | Right Rear Window Switch | Driver Door Module, Passenger Door Module | DTC B316B, B317A, B318A, or B319A
B3205 | Driver Window Motor Circuit | Driver Door Module, Passenger Door Module | DTC B3205, B3210, B3215, or B3220
B3210 | Passenger Window Motor Circuit | Driver Door Module, Passenger Door Module | DTC B3205, B3210, B3215, or B3220
B3215 | Left Rear Window Motor Circuit | Driver Door Module, Passenger Door Module | DTC B3205, B3210, B3215, or B3220
B3220 | Right Rear Window Motor Circuit | Driver Door Module, Passenger Door Module | DTC B3205, B3210, B3215, or B3220
B3265 | Trunk Lid Unlatch Output Circuit | BCM | DTC B3265
B3445 | Brake Lamps Circuit | BCM | DTC B3445 or B3878
B3567 | Driver Information Center Switch Circuit | Instrument Cluster | DTC B3567
B3588 | Rear Fog Lamp Switch Circuit | BCM | DTC B3588
B3596 | Hazard Lamps Request Circuit | BCM | DTC B3596
B3622 | Steering Wheel Controls Signal Circuit | BCM | DTC B3622
B3650 | High Beam Request Signal Circuit | BCM | DTC B3650
B370A | Rain Sensor | BCM | DTC B370A
B3715 | Front Wiper Relay Circuit | BCM | DTC B3715 or B3875
B3794 | Cruise Control Function Request Circuit | BCM | DTC B3794
B3806 | High Beam and Headlamp Flash Select Circuit | BCM | DTC B3806
B3867 | Right Park Lamps Control Circuit | BCM | DTC B2585 or B3867
B3873 | Front Washer Relay Circuit | BCM | DTC B3873
B3875 | Windshield Wiper High Speed Relay Circuit | BCM | DTC B3715 or B3875
B3878 | Right Brake Lamp Circuit | BCM | DTC B3445 or B3878
B3883 | License Plate Lamp Circuit | BCM | DTC B3883
B3884 | Center High Mounted Brake Lamp Circuit | BCM | DTC B3884
B3902 | Incorrect Immobilizer Identifier Received | BCM | DTC B3902
B3933 | Air Conditioning Evaporator Temperature Sensor Circuit | Heater and Blower and Air Conditioning Control Module | DTC B0173, B0178, or B3933 for the automatic system or DTC B3933 for the manual system
B3935 | Transponder Authentication Error | BCM | DTC B3935
B3948 | Left Front Turn Signal Circuit | BCM | DTC B3948 or B3949
B3949 | Right Front Turn Signal Circuit | BCM | DTC B3948 or B3949
B3950 | Left Rear Turn Signal Circuit | BCM | DTC B3950 or B3951
B3951 | Right Rear Turn Signal Circuit | BCM | DTC B3950 or B3951
B3976 | Unconfigured Transponder | BCM | DTC B3976
B3984 | Device 1 Environment Identifier Not Programmable | BCM | DTC B3984
C0035 | Left Front Wheel Speed Sensor Circuit | EBCM | DTC C0035, C0040, C0045, or C0050
C0040 | Right Front Wheel Speed Sensor Circuit | EBCM | DTC C0035, C0040, C0045, or C0050
C0045 | Left Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035, C0040, C0045, or C0050
C0050 | Right Rear Wheel Speed Sensor Circuit | EBCM | DTC C0035, C0040, C0045, or C0050
C0110 | Pump Motor Circuit | EBCM | DTC C0110
C0131 | Traction Control System Pressure Circuit | EBCM | DTC C0131
C0161 | Antilock Braking System Brake Switch Circuit | EBCM | DTC C0161
C0186 | Lateral Acceleration Sensor Circuit | EBCM | DTC C0186, C0196, or C019B
C0196 | Yaw Rate Circuit | EBCM | DTC C0186, C0196, or C019B
C019B | Yaw Rate Signal | EBCM | DTC C0186, C0196, or C019B
C0267 | Low Brake Fluid Indicated | EBCM | DTC C0267
C0280 | Stability System Active Too Long | EBCM | DTC C0280
C0550 | Electronic Control Unit | EBCM | DTC C0550
C056D | Electronic Control Unit Hardware | EBCM | DTC C056D
C056E | Electronic Control Unit Software | EBCM | DTC C056E
C0710 | Steering Position Signal | EBCM | DTC C0710
C0800 | Control Module Power Circuit | EBCM | DTC C0800
P000A | Intake Camshaft Position System Slow Response | ECM | DTC P000A, P000B, P0011, or P0014
P000B | Exhaust Camshaft Position System Slow Response | ECM | DTC P000A, P000B, P0011, or P0014
P0010 | Intake Camshaft Position Actuator Solenoid Control Circuit | ECM | DTC P0010, P0013, or P2088-P2091
P0011 | Intake Camshaft Position System Performance | ECM | DTC P000A, P000B, P0011, or P0014
P0013 | Exhaust Camshaft Position Actuator Solenoid Control Circuit | ECM | DTC P0010, P0013, or P2088-P2091
P0014 | Exhaust Camshaft Position System Performance | ECM | DTC P000A, P000B, P0011, or P0014
P0016 | Crankshaft Position - Intake Camshaft Position Not Plausible | ECM | DTC P0016 or P0017 for the 1.6L engine
Crankshaft Position - Camshaft Position Correlation Not Plausible | DTC P0016 for the 2.0L engine
P0017 | Crankshaft Position - Exhaust Camshaft Position Not Plausible | ECM | DTC P0016 or P0017
P0030 | HO2S Heater Control Circuit Sensor 1 | ECM | DTC P0030-P0032, or P0135
P0031 | HO2S Heater Control Circuit Low Voltage Sensor 1 | ECM | DTC P0030-P0032, or P0135
P0032 | HO2S Heater Control Circuit High Voltage Sensor 1 | ECM | DTC P0030-P0032, or P0135
P0036 | HO2S Heater Control Circuit Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141
P0037 | HO2S Heater Control Circuit Low Voltage Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141
P0038 | HO2S Heater Control Circuit High Voltage Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141
P0045 | Turbocharger Boost Control Solenoid Control Circuit | ECM | DTC P0045
P0068 | Throttle Body Airflow Performance | ECM | DTC P0068, P0121, or P0221
P0069 | Manifold Absolute Pressure - Barometric Pressure Correlation | ECM | DTC P0069
P0089 | Fuel Pressure Regulator Performance | ECM | DTC P0089
P0090 | Fuel Pressure Regulator Solenoid 1 Control Circuit | ECM | DTC P0090
P0095 | Intake Air Temperature Sensor 2 Circuit | ECM | DTC P0095
P00B3 | Radiator Coolant Temperature Sensor Circuit Low Voltage | ECM | DTC P00B3 or P00B4
P00B4 | Radiator Coolant Temperature Sensor Circuit High Voltage | ECM | DTC P00B3 or P00B4
P0100 | Mass Air Flow Sensor Circuit | ECM | DTC P0100
P0101 | Mass Air Flow Sensor Performance | ECM | DTC P0101
P0105 | Manifold Absolute Pressure Sensor Circuit | ECM | DTC P0105
P0106 | Manifold Absolute Pressure Sensor Performance | ECM | DTC P0106, P0107, or P0108
P0107 | Manifold Absolute Pressure Sensor Circuit Low Voltage | ECM | DTC P0106, P0107, or P0108
P0108 | Manifold Absolute Pressure Sensor Circuit High Voltage | ECM | DTC P0106, P0107, or P0108
P0110 | Intake Air Temperature Sensor 1 Circuit | ECM | DTC P0110
P0111 | Intake Air Temperature Sensor Performance | ECM | DTC P0111-P0113
P0112 | Intake Air Temperature Sensor Circuit Low Voltage | ECM | DTC P0111-P0113
P0113 | Intake Air Temperature Sensor Circuit High Voltage | ECM | DTC P0111-P0113
P0114 | Intake Air Temperature Sensor Circuit Intermittent | ECM | DTC P0114
P0115 | Engine Coolant Temperature Sensor Circuit | ECM | DTC P0115
P0116 | Engine Coolant Temperature Sensor Performance | ECM | DTC P0116 for the 1.6L engine or DTC P0116 for the 2.0L engine
P0117 | Engine Coolant Temperature Sensor Circuit Low Voltage | ECM | DTC P0117, P0118, or P0119
P0118 | Engine Coolant Temperature Sensor Circuit High Voltage | ECM | DTC P0117, P0118, or P0119
P0119 | Engine Coolant Temperature Sensor Circuit Intermittent | ECM | DTC P0117, P0118, or P0119
P0121 | Throttle Position Sensor 1 Performance | ECM | DTC P0068, P0121, or P0221
P0122 | Throttle Position Sensor 1 Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, or P0223
P0123 | Throttle Position Sensor 1 Circuit High Voltage | ECM | DTC P0122, P0123, P0222, or P0223
P0128 | Engine Coolant Temperature Below Thermostat Regulating Temperature | ECM | DTC P0128
P0130 | HO2S Circuit Sensor 1 | ECM | DTC P0130-P0134 or P2A00
P0131 | HO2S Circuit Low Voltage Sensor 1 | ECM | DTC P0130-P0134 or P2A00
P0132 | HO2S Circuit High Voltage Sensor 1 | ECM | DTC P0130-P0134 or P2A00
P0133 | HO2S Slow Response Sensor 1 | ECM | DTC P0130-P0134 or P2A00
P0134 | HO2S Circuit Insufficient Activity Sensor 1 | ECM | DTC P0130-P0134 or P2A00
P0135 | HO2S Heater Performance Sensor 1 | ECM | DTC P0030-P0032, or P0135
P0136 | HO2S Circuit Sensor 2 | ECM | DTC P0136
P0137 | HO2S Circuit Low Voltage Sensor 2 | ECM | DTC P0137-P0140, P2270, P2271, or P2A01
P0138 | HO2S Circuit High Voltage Sensor 2 | ECM | DTC P0137-P0140, P2270, P2271, or P2A01
P0139 | HO2S Circuit Slow Response Sensor 2 | ECM | DTC P0137-P0140, P2270, P2271, or P2A01
P0140 | HO2S Circuit Insufficient Activity Sensor 2 | ECM | DTC P0137-P0140, P2270, P2271, or P2A01
P0141 | HO2S Heater Performance Sensor 2 | ECM | DTC P0036, P0037, P0038, or P0141
P0171 | Fuel Trim System Lean | ECM | DTC P0171 or P2096
P0172 | Fuel Trim System Rich | ECM | DTC P0172 or P2097
P0180 |  | ECM | DTC P0180
P0190 | Fuel Rail Pressure Sensor Circuit | ECM | DTC P0190 or P0191
P0191 | Fuel Rail Pressure Sensor Performance | ECM | DTC P0190 or P0191
P0201 | Cylinder 1 Injector Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine
Fuel Injector 1 Control Circuit | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L engine
P0202 | Cylinder 2 Injector Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine
Fuel Injector 2 Control Circuit | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L engine
P0203 | Cylinder 3 Injector Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine
Fuel Injector 3 Control Circuit | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L engine
P0204 | Cylinder 4 Injector Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271 for the 1.6L engine
Fuel Injector 4 Control Circuit | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233 for the 2.0L engine
P0218 | Transmission Fluid Overtemperature | TCM | DTC P0218
P0219 | Engine Overspeed | ECM | DTC P0219
P0221 | Throttle Position Sensor 2 Performance | ECM | DTC P0068, P0121, or P0221
P0222 | Throttle Position Sensor 2 Circuit Low Voltage | ECM | DTC P0122, P0123, P0222, or P0223
P0223 | Throttle Position Sensor 2 Circuit High Voltage | ECM | DTC P0122, P0123, P0222, or P0223
P0234 | Turbocharger Engine Overboost | ECM | DTC P0234 or P0299
P0261 | Cylinder 1 Injector Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0262 | Cylinder 1 Injector Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0263 | Cylinder 1 Balance System | ECM | DTC P0263, P0266, P0269, or P0272
P0264 | Cylinder 2 Injector Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0265 | Cylinder 2 Injector Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0266 | Cylinder 2 Balance System | ECM | DTC P0263, P0266, P0269, or P0272
P0267 | Cylinder 3 Injector Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0268 | Cylinder 3 Injector Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0269 | Cylinder 3 Balance System | ECM | DTC P0263, P0266, P0269, or P0272
P0270 | Cylinder 4 Injector Control Circuit Low Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0271 | Cylinder 4 Injector Control Circuit High Voltage | ECM | DTC P0201, P0202, P0203, P0204, P0261, P0262, P0264, P0265, P0267, P0268, P0270, or P0271
P0272 | Cylinder 4 Balance System | ECM | DTC P0263, P0266, P0269, or P0272
P0299 | Turbocharger Engine Underboost | ECM | DTC P0234 or P0299
P02E0 | Intake Air Flow Valve Control Circuit | ECM | DTC P02E0
P02E1 | Intake Air Flow Valve Control Performance | ECM | DTC P02E1
P0300 | Engine Misfire Detected | ECM | DTC P0300-P0304 or P0313
P0301 | Cylinder 1 Misfire Detected | ECM | DTC P0300-P0304 or P0313
P0302 | Cylinder 2 Misfire Detected | ECM | DTC P0300-P0304 or P0313
P0303 | Cylinder 3 Misfire Detected | ECM | DTC P0300-P0304 or P0313
P0304 | Cylinder 4 Misfire Detected | ECM | DTC P0300-P0304 or P0313
P0313 | Misfire Detected With Low Fuel Level | ECM | DTC P0300-P0304 or P0313
P0318 | Rough Road Sensor Circuit | ECM | DTC P0318
P0325 | Knock Sensor 1 Circuit | ECM | DTC P0325 or P0326
P0326 | Knock Sensor Performance | ECM | DTC P0325 or P0326
P0335 | Crankshaft Position Sensor Circuit | ECM | DTC P0335 or P0336 for the 1.6L engine or DTC P0335 for the 2.0L engine
P0336 | Crankshaft Position Sensor Performance | ECM | DTC P0335 or P0336
P0340 | Intake Camshaft Position Sensor Circuit | ECM | DTC P0340, P0341, P0365, or P0366 for the 1.6L engine
Camshaft Position Sensor Circuit | DTC P0340 for the 2.0L engine
P0341 | Intake Camshaft Position Sensor Performance | ECM | DTC P0340, P0341, P0365, or P0366
P0365 | Exhaust Camshaft Position Sensor Circuit | ECM | DTC P0340, P0341, P0365, or P0366
P0366 | Exhaust Camshaft Position Sensor Performance | ECM | DTC P0340, P0341, P0365, or P0366
P0381 | Wait to Start Lamp Control Circuit | ECM | DTC P0381
P0401 | Exhaust Gas Recirculation Flow Insufficient | ECM | DTC P0401 or P0402
P0402 | Exhaust Gas Recirculation Flow Excessive | ECM | DTC P0401 or P0402
P0403 | Exhaust Gas Recirculation Solenoid Control Circuit | ECM | DTC P0403
P0420 | Catalyst System Low Efficiency | ECM | DTC P0420
P0442 | Evaporative Emissions System Small Leak Detected | ECM | DTC P0442 or P0456
P0443 | Evaporative Emission Purge Solenoid Valve Control Circuit | ECM | DTC P0443, P0458, or P0459
P0446 | Evaporative Emissions Vent System Performance | ECM | DTC P0446
P0451 | Fuel Tank Pressure Sensor Performance | ECM | DTC P0451, P0452, P0453, or P0454
P0452 | Fuel Tank Pressure Sensor Circuit Low Voltage | ECM | DTC P0451, P0452, P0453, or P0454
P0453 | Fuel Tank Pressure Sensor Circuit High Voltage | ECM | DTC P0451, P0452, P0453, or P0454
P0454 | Fuel Tank Pressure Sensor Circuit Intermittent | ECM | DTC P0451, P0452, P0453, or P0454
P0455 | Evaporative Emission System Large Leak | ECM | DTC P0455
P0456 | Evaporative Emission System Large Leak Detected | ECM | DTC P0442 or P0456
P0458 | Evaporative Emission Purge Solenoid Control Circuit Low Voltage | ECM | DTC P0443, P0458, or P0459
P0459 | Evaporative Emission Purge Solenoid Control Circuit High Voltage | ECM | DTC P0443, P0458, or P0459
P0461 | Fuel Level Sensor Circuit Performance | ECM | DTC P0461-P0463
P0462 | Fuel Level Sensor Circuit Low Voltage | ECM | DTC P0461-P0463
P0463 | Fuel Level Sensor Circuit High Voltage | ECM | DTC P0461-P0463
P0480 | Cooling Fan Relay 1 Control Circuit | ECM | DTC P0480, P0481, or P0482
P0481 | Cooling Fan Relay 2 Control Circuit | ECM | DTC P0480, P0481, or P0482
P0482 | Cooling Fan Relay 3 Control Circuit | ECM | DTC P0480, P0481, or P0482
P0496 | Evaporative Emission System Flow During Non-Purge | ECM | DTC P0496
P0498 | Evaporative Emission Vent Solenoid Control Circuit Low Voltage | ECM | DTC P0498 or P0499
P0499 | Evaporative Emission Vent Solenoid Control Circuit High Voltage | ECM | DTC P0498 or P0499
P0506 | Idle Speed Low | ECM | DTC P0506 or P0507
P0507 | Idle Speed High | ECM | DTC P0506 or P0507
P050A | Cold Start Idle Air Control System Performance | ECM | DTC P050A
P0513 | Immobilizer Key Incorrect | ECM | DTC P0513
P0520 | Engine Oil Pressure Switch Circuit Malfunction | ECM | DTC P0520
P0530 | Air Conditioning Refrigerant Pressure Sensor Circuit | ECM | DTC P0530, P0532, or P0533 for the automatic system or DTC P0530, P0532, or P0533 for the manual system
P0532 | Air Conditioning Pressure Sensor Circuit Low Voltage | ECM | DTC P0530, P0532, or P0533 for the automatic system or DTC P0530, P0532, or P0533 for the manual system
P0533 | Air Conditioning Pressure Sensor Circuit High Voltage | ECM | DTC P0530, P0532, or P0533 for the automatic system or DTC P0530, P0532, or P0533 for the manual system
P0544 | Exhaust Gas Temperature Sensor 1 Circuit | ECM | DTC P0544 or P2031
P0560 | System Voltage | ECM | DTC P0560
P0562 | System Voltage Low | ECM | DTC P0562
TCM | DTC P0562 or P0563
P0563 | System Voltage High | ECM | DTC P0563
TCM | DTC P0562 or P0563
P0564 | Cruise Control Multi-Function Switch Circuit | BCM | DTC P0564
P0571 | Brake Switch Circuit | BCM | DTC P0571
P0597 | Engine Coolant Thermostat Heater Control Circuit | ECM | DTC P0597-P0599
P0598 | Engine Coolant Thermostat Heater Control Circuit Low Voltage | ECM | DTC P0597-P0599
P0599 | Engine Coolant Thermostat Heater Control Circuit High Voltage | ECM | DTC P0597-P0599
P0601 | Control Module Read Only Memory | ECM | DTC P0601, P0602, P0604, P0606, P0607, P061A, or P2610 for the 1.6L engine
Transmission Control Module Read Only Memory | TCM | DTC P0601-P0604 or P062F
P0602 | Control Module Not Programmed | ECM | DTC P0601, P0602, P0604, P0606, P0607, P061A, or P2610 for the 1.6L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine
Transmission Control Module Not Programmed | TCM | DTC P0601-P0604 or P062F
P0603 | Transmission Control Module Long Term Memory Reset | TCM | DTC P0601-P0604 or P062F
P0604 | Control Module Random Access Memory | ECM | DTC P0601, P0602, P0604, P0606, P0607, P061A, or P2610
Transmission Control Module Random Access Memory | TCM | DTC P0601-P0604 or P062F
P0606 | Control Module Internal Performance | ECM | DTC P0601, P0602, P0604, P0606, P0607, P061A, or P2610 for the 1.6L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine
P0607 | Control Module Performance | ECM | DTC P0601, P0602, P0604, P0606, P0607, P061A, or P2610 for the 1.6L engine or DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F for the 2.0L engine
P060A | Control Module Monitoring Processor Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
P060B | Control Module Analog to Digital Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
P0615 | Starter Relay Control Circuit | ECM | DTC P0615
P0616 | Starter Relay Control Circuit Low Voltage | ECM | DTC P0616
P0617 | Starter Relay Control Circuit High Voltage | ECM | DTC P0617
P061A | Control Module Long Term Memory Performance | ECM | DTC P0601, P0602, P0604, P0606, P0607, P061A, or P2610
P061C | Control Module Engine Speed Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
P0621 | Generator L-Terminal Circuit | ECM | DTC P0621
P0622 | Generator F-Terminal Circuit | ECM | DTC P0622
P0627 | Fuel Pump Relay Control Circuit | ECM | DTC P0627
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0628 or P0629
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0628 or P0629
P062B | Control Module Fuel Injector Control Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
P062F | Control Module Long Term Memory Performance | ECM | DTC P0601, P0602, P0603, P0604, P0605, P0606, P0607, P060A, P060B, P061C, P062B, or P062F
Transmission Control Module Long Term Memory Performance | TCM | DTC P0601-P0604 or P062F
P0630 | VIN Not Programmed or Mismatched - Engine Control Module | ECM | DTC P0630
P0633 | Immobilizer Key Not Programmed | ECM | DTC P0633
P0634 | Transmission Control Module Overtemperature | TCM | DTC P0634
P0641 | 5-Volt Reference 1 Circuit | ECM | DTC P0641, P0651, or P0697
P0642 | 5-Volt Reference 1 Low Voltage | ECM | DTC P0642, P0643, P0652, or P0653
P0643 | 5-Volt Reference 1 High Voltage | ECM | DTC P0642, P0643, P0652, or P0653
P0645 | Air Conditioning Clutch Relay Control Circuit | ECM | DTC P0645, P0646, or P0647 for the automatic system or DTC P0645, P0646, or P0647 for the manual system
P0646 | Air Conditioning Clutch Relay Control Circuit Low Voltage | ECM | DTC P0645, P0646, or P0647 for the automatic system or DTC P0645, P0646, or P0647 for the manual system
P0647 | Air Conditioning Clutch Relay Control Circuit High Voltage | ECM | DTC P0645, P0646, or P0647 for the automatic system or DTC P0645, P0646, or P0647 for the manual system
P0649 | Cruise Engaged Lamp Control Circuit | ECM | DTC P0649
P064C | Glow Plug Control Module Performance | ECM | DTC P0649
P0650 | Malfunction Indicator Lamp Control Circuit | ECM | DTC P0650 for the 1.6L engine or DTC P0650 for the 2.0L engine
P0651 | 5-Volt Reference 2 Circuit | ECM | DTC P0641, P0651, or P0697
P0652 | 5-Volt Reference 2 Low Voltage | ECM | DTC P0642, P0643, P0652, or P0653
P0653 | 5-Volt Reference 2 High Voltage | ECM | DTC P0642, P0643, P0652, or P0653
P0655 | Engine Coolant Temperature Lamp Control Circuit | ECM | DTC P0655
P0658 | Pressure Control/Shift Lock Solenoid Control Circuit Low Voltage | TCM | DTC P0658 or P0659
P0659 | Pressure Control/Shift Lock Solenoid Control Circuit High Voltage | TCM | DTC P0658 or P0659
P065E | Intake Manifold Tuning Control Valve Performance | ECM | DTC P065E
P0661 | Intake Manifold Tuning Valve Solenoid Control Circuit Low Voltage | ECM | DTC P0661 or P0662
P0662 | Intake Manifold Tuning Valve Solenoid Control Circuit High Voltage | ECM | DTC P0661 or P0662
P0667 | Transmission Control Module Temperature Sensor Performance | TCM | DTC P0667, P0668, or P0669
P0668 | Transmission Control Module Temperature Sensor Circuit Low Voltage | TCM | DTC P0667, P0668, or P0669
P0669 | Transmission Control Module Temperature Sensor Circuit High Voltage | TCM | DTC P0667, P0668, or P0669
P0670 | Glow Plug Control Module Control Circuit | ECM | DTC P0670
P0671 | Glow Plug 1 Control Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0672 | Glow Plug 2 Control Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0673 | Glow Plug 3 Control Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0674 | Glow Plug 4 Control Circuit | ECM | DTC P0671, P0672, P0673, or P0674
P0683 | Glow Plug Control Module Communication Circuit | ECM | DTC P0683
P0691 | Cooling Fan Relay 1 Control Circuit Low Voltage | ECM | DTC P0691-P0694
P0692 | Cooling Fan Relay 1 Control Circuit High Voltage | ECM | DTC P0691-P0694
P0693 | Cooling Fan Relay 2 Control Circuit Low Voltage | ECM | DTC P0691-P0694
P0694 | Cooling Fan Relay 2 Control Circuit High Voltage | ECM | DTC P0691-P0694
P0697 | 5-Volt Reference 3 Circuit | ECM | DTC P0641, P0651, or P0697
P06AC | Transmission Control Module Power Up Temperature Sensor Performance | TCM | DTC P0667, P0668, or P0669
P06AD | Transmission Control Module Power Up Temperature Sensor Circuit Low Voltage | TCM | DTC P0667, P0668, or P0669
P06AE | Transmission Control Module Power Up Temperature Sensor Circuit High Voltage | TCM | DTC P0667, P0668, or P0669
P0700 | Transmission Control Module Requested MIL Illumination | ECM | DTC P0700 for the 1.6L engine or DTC P0700 for the 2.0L engine
P0703 | Cruise Control Brake Switch Circuit | BCM | DTC P0703
P0711 | Transmission Fluid Temperature Sensor Performance | TCM | DTC P0711, P0712, or P0713
P0712 | Transmission Fluid Temperature Sensor Circuit Low Voltage | TCM | DTC P0711, P0712, or P0713
P0713 | Transmission Fluid Temperature Sensor Circuit High Voltage | TCM | DTC P0711, P0712, or P0713
P0716 | Input Speed Sensor Performance | TCM | DTC P0716 or P0717
P0717 | Input Speed Sensor Circuit Low Voltage | TCM | DTC P0716 or P0717
P071A | Transmission Tow Mode Switch Circuit | TCM | DTC P071A
P071D | Trans Mode Switch B circuit | TCM | DTC P071D
P0722 | Output Speed Sensor Circuit Low Voltage | TCM | DTC P0722 or P0723
P0723 | Output Speed Sensor Circuit Intermittent | TCM | DTC P0722 or P0723
P0741 | Torque Converter Clutch - Stuck Off | TCM | DTC P0741 or P0742
P0742 | Torque Converter Clutch - Stuck On | TCM | DTC P0741 or P0742
P0751 | Shift Solenoid 1 Valve Performance - Stuck Off | TCM | DTC P0751
P0752 | Shift Solenoid 1 Valve Performance - Stuck On | TCM | DTC P0752
P0756 | Shift Solenoid 2 Valve Performance - Stuck Off | TCM | DTC P0756
P0776 | Clutch Pressure Control Solenoid 2 - Stuck Off | TCM | DTC P0776 or P0777
P0777 | Clutch Pressure Control Solenoid 3 - Stuck On | TCM | DTC P0776 or P0777
P0796 | Clutch Pressure Control Solenoid 3 - Stuck Off | TCM | DTC P0796 or P0797
P0797 | Clutch Pressure Control Solenoid 2 - Stuck On | TCM | DTC P0796 or P0797
P0815 | Upshift Switch Circuit | TCM | DTC P0815, P0816, or P0826
P0816 | Downshift Switch Circuit | TCM | DTC P0815, P0816, or P0826
P0826 | Up and Down Shift Switch Circuit | TCM | DTC P0815, P0816, or P0826
P0842 | Transmission Fluid Pressure Switch 1 Circuit Low Voltage | TCM | DTC P0842, P0843, P0872, P0873, P0877, P0878, P0989, or P0990
P0843 | Transmission Fluid Pressure Switch 1 Circuit High Voltage | TCM | DTC P0842, P0843, P0872, P0873, P0877, P0878, P0989, or P0990
P0872 | Transmission Fluid Pressure Switch 3 Circuit Low Voltage | TCM | DTC P0842, P0843, P0872, P0873, P0877, P0878, P0989, or P0990
P0873 | Transmission Fluid Pressure Switch 3 Circuit High Voltage | TCM | DTC P0842, P0843, P0872, P0873, P0877, P0878, P0989, or P0990
P0877 | Transmission Fluid Pressure Switch 4 Circuit Low Voltage | TCM | DTC P0842, P0843, P0872, P0873, P0877, P0878, P0989, or P0990
P0878 | Transmission Fluid Pressure Switch 4 Circuit High Voltage | TCM | DTC P0842, P0843, P0872, P0873, P0877, P0878, P0989, or P0990
P0850 | Park/Neutral Position Switch Circuit | TCM | DTC P0850-P0852
P0851 | Park/Neutral Position Switch Circuit Low Voltage | TCM | DTC P0850-P0852
P0852 | Park/Neutral Position Switch Circuit High Voltage | TCM | DTC P0850-P0852
P0856 | Traction Control Torque Request Circuit Malfunction | ECM | DTC P0856
P0961 | Line Pressure Control Solenoid System Performance | TCM | DTC P0961-P0963
P0962 | Line Pressure Control Solenoid Circuit Low Voltage | TCM | DTC P0961-P0963
P0963 | Line Pressure Control Solenoid Circuit High Voltage | TCM | DTC P0961-P0963
P0965 | Clutch Pressure Control Solenoid 2 System Performance | TCM | DTC P0965-P0967
P0966 | Clutch Pressure Control Solenoid 2 Circuit Low Voltage | TCM | DTC P0965-P0967
P0967 | Clutch Pressure Control Solenoid 2 Circuit High Voltage | TCM | DTC P0965-P0967
P0696 | Clutch Pressure Control Solenoid 3 System Performance | TCM | DTC P0969-P0971
P0970 | Clutch Pressure Control Solenoid 3 Circuit Low Voltage | TCM | DTC P0969-P0971
P0971 | Clutch Pressure Control Solenoid 3 Circuit High Voltage | TCM | DTC P0969-P0971
P0973 | Shift Solenoid 1 Control Circuit Low Voltage | TCM | DTC P0973 or P0974
P0974 | Shift Solenoid 1 Control Circuit High Voltage | TCM | DTC P0973 or P0974
P0989 | Transmission Fluid Pressure Switch 5 Circuit Low Voltage | TCM | DTC P0842, P0843, P0872, P0873, P0877, P0878, P0989, or P0990
P0990 | Transmission Fluid Pressure Switch 5 Circuit High Voltage | TCM | DTC P0842, P0843, P0872, P0873, P0877, P0878, P0989, or P0990
P1224 | Fuel Injector 1 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233
P1227 | Fuel Injector 2 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233
P122A | Fuel Injector 3 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233
P1233 | Fuel Injector 4 Control Circuit | ECM | DTC P0201, P0202, P0203, P0204, P1224, P1227, P122A, or P1233
P1336 | Crankshaft Position System Variation Not Learned | ECM | DTC P1336
P1446 | Pre-Catalyst Temperature Too Low During Regeneration | ECM | DTC P1446 or P1447
P1447 | Pre-Catalyst Temperature Too High During Regeneration | ECM | DTC P1446 or P1447
P161C | Tire Size Not Programmed | ECM | DTC P161C
P161E | Glow Plug Positive Voltage Circuit | ECM | DTC P161E
P161F | Assembly Plant Mode Counter Not Programmed | ECM | DTC P161F
P1629 | Immobilizer Fuel Enable Signal Not Received | ECM | DTC P1629
P1631 | Theft Deterrent Fuel Enable Signal Not Correct | ECM | DTC P1631
P1632 | Immobilizer Fuel Disable Signal Received | ECM | DTC P1632
P1649 | Immobilizer Security Code Not Programmed | ECM | DTC P1649
P1663 | Change Oil Lamp Control Circuit | ECM | DTC P1663
P1678 | Immobilizer System - Incorrect Engine Control Module Identification | ECM | DTC P1678
P1691 | Engine Coolant Temperature Output Circuit | ECM | DTC P1691
P1751 | Shift Valve 1 Performance | TCM | DTC P1751
P1761 | Tap Up and Down Switch Signal Circuit | TCM | DTC P1761 or P1762
P1762 | Trans Mode Switch Signal Circuit | TCM | DTC P1761 or P1762
P1763 | Trans Mode Switch Circuit | TCM | DTC P1763
P1793 | Wheel Speed Signal | ECM | DTC P1793
P1825 | Internal Mode Switch - Invalid Range | TCM | DTC P1825, P182E, or P1915
P182E | Internal Mode Switch - Invalid Range | TCM | DTC P1825, P182E, or P1915
P1876 | Up and Down Shift Enable Switch Circuit Low Voltage | TCM | DTC P1876
P1915 | Internal Mode Switch Does Not Indicate Park/Neutral During Start | TCM | DTC P1825, P182E, or P1915
P2002 | Diesel Particulate Filter Low Efficiency | ECM | DTC P2002
P2031 | Exhaust Gas Temperature Sensor 2 Circuit | ECM | DTC P0544 or P2031
P2072 | Throttle Actuator Control System Ice Blockage | ECM | DTC P2072
P2080 | Exhaust Gas Temperature Sensor 1 | ECM | DTC P2080 or P2084
P2084 | Exhaust Gas Temperature Sensor 2 | ECM | DTC P2080 or P2084
P2088 | Intake Camshaft Position Actuator Solenoid Control Circuit Low Voltage | ECM | DTC P0010, P0013, or P2088-P2091
P2089 | Intake Camshaft Position Actuator Solenoid Control Circuit High Voltage | ECM | DTC P0010, P0013, or P2088-P2091
P2090 | Exhaust Camshaft Position Actuator Solenoid Control Circuit Low Voltage | ECM | DTC P0010, P0013, or P2088-P2091
P2091 | Exhaust Camshaft Position Actuator Solenoid Control Circuit High Voltage | ECM | DTC P0010, P0013, or P2088-P2091
P2096 | Fuel Trim System Low Limit | ECM | DTC P0171 or P2096
P2097 | Fuel Trim System High Limit | ECM | DTC P0172 or P2097
P2100 | Throttle Actuator Control Motor Control Circuit | ECM | DTC P2100, P2101, P2108, P2119, or P2176
P2101 | Control Module Throttle Actuator Position Performance | ECM | DTC P2100, P2101, P2108, P2119, or P2176
P2108 | Throttle Actuator Control Module Performance | ECM | DTC P2100, P2101, P2108, P2119, or P2176
P2119 | Throttle Closed Position Performance | ECM | DTC P2100, P2101, P2108, P2119, or P2176
P2120 | Accelerator Pedal Position Sensor 1 Circuit Malfunction | ECM | DTC P2120, P2125, or P2138
P2122 | Accelerator Pedal Position Sensor 1 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2123 | Accelerator Pedal Position Sensor 1 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2125 | Accelerator Pedal Position Sensor 2 Circuit Voltage | ECM | DTC P2120, P2125, or P2138
P2127 | Accelerator Pedal Position Sensor 2 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2128 | Accelerator Pedal Position Sensor 2 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2138 | Accelerator Pedal Position Sensor 1-2 Correlation | ECM | DTC P2122, P2123, P2127, P2128, or P2138 for the 1.6L engine or DTC P2120, P2125, or P2138 for the 2.0L engine
P2146 | Injector Positive Voltage Control Circuit Group 1 | ECM | DTC P2146 or P2149
P2149 | Injector Positive Voltage Control Circuit Group 2 | ECM | DTC P2146 or P2149
P2176 | Minimum Throttle Position Not Learned | ECM | DTC P2100, P2101, P2108, P2119, or P2176
P2226 | Barometric Pressure Sensor Circuit Voltage | ECM | DTC P2226
P2270 | HO2S Signal Stuck Lean Sensor 2 | ECM | DTC P0137-P0140, P2270, P2271, or P2A01
P2271 | HO2S Signal Stuck Rich Sensor 2 | ECM | DTC P0137-P0140, P2270, P2271, or P2A01
P2297 | HO2S Performance During Decel Fuel Cut-Off Sensor 1 | ECM | DTC P2297
P2300 | Ignition Coil 1 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2301 | Ignition Coil 1 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2303 | Ignition Coil 2 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2304 | Ignition Coil 2 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2306 | Ignition Coil 3 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2307 | Ignition Coil 3 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2309 | Ignition Coil 4 Control Circuit Low Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P2310 | Ignition Coil 4 Control Circuit High Voltage | ECM | DTC P2300, P2301, P2303, P2304, P2306, P2307, P2309, or P2310
P244B | Diesel Particulate Filter Differential Pressure | ECM | DTC P244B
P244C | Catalyst Temperature Too Low During Regeneration | ECM | DTC P244C
P2452 | Diesel Particulate Filter Differential Pressure Sensor Circuit | ECM | DTC P2452
P2453 | Diesel Particulate Filter Differential Pressure Sensor Performance | ECM | DTC P2453
P2458 | Diesel Particulate Filter Regeneration Time | ECM | DTC P2458
P2463 | Diesel Particulate Filter Soot Accumulation | ECM | DTC P2463
P2510 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P2510
P2533 | Ignition 1 Switch Circuit | ECM | DTC P2533
P2534 | Ignition 1 Switch Circuit Low Voltage | TCM | DTC P2534
P2544 | Transmission Torque Request Circuit | ECM | DTC P2544
P260E | Diesel Particulate Filter Lamp Control Circuit | ECM | DTC P260E
P2610 | Control Module Ignition Off Timer Performance | ECM | DTC P0601, P0602, P0604, P0606, P0607, P061A, or P2610
P2687 | Fuel Heater Relay Control Circuit | ECM | DTC P2687
P268A | Fuel Injector Calibration Data Not Programmed | ECM | DTC P268A
P2714 | Clutch Pressure Control Solenoid 4 - Stuck Off | TCM | DTC P2714 or P2715
P2715 | Clutch Pressure Control Solenoid 4 - Stuck On | TCM | DTC P2714 or P2715
P2719 | Clutch Pressure Control Solenoid 4 - System Performance | TCM | DTC P2719-P2721
P2720 | Clutch Pressure Control Solenoid 4 - Low Voltage | TCM | DTC P2719-P2721
P2721 | Clutch Pressure Control Solenoid 4 - High Voltage | TCM | DTC P2719-P2721
P2723 | Clutch Pressure Control Solenoid 5 - Stuck Off | TCM | DTC P2723 or P2724
P2724 | Clutch Pressure Control Solenoid 5 - Stuck On | TCM | DTC P2723 or P2724
P2728 | Clutch Pressure Control Solenoid 5 - System Performance | TCM | DTC P2728-P2730
P2729 | Clutch Pressure Control Solenoid 5 - Low Voltage | TCM | DTC P2728-P2730
P2730 | Clutch Pressure Control Solenoid 5 - High Voltage | TCM | DTC P2728-P2730
P2762 | Torque Converter Clutch Pressure Control Solenoid System Performance | TCM | DTC P2762, P2763, or P2764
P2763 | Torque Converter Clutch Pressure Control Solenoid Control Circuit High Voltage | TCM | DTC P2762, P2763, or P2764
P2764 | Torque Converter Clutch Pressure Control Solenoid Control Circuit Low Voltage | TCM | DTC P2762, P2763, or P2764
P2A00 | HO2S Circuit Closed Loop Performance Sensor 1 | ECM | DTC P0130-P0134 or P2A00
P2A01 | HO2S Performance During Decel Fuel Cut-Off Sensor 2 | ECM | DTC P0137-P0140, P2270, P2271, or P2A01
U0002 | High Speed Controller Area Network Communication Bus Performance | -- | DTC U0002
U0020 | Low Speed Controller Area Network Communication Bus Performance | -- | DTC U0020
U0073 | Control Module Communication Bus Off | -- | DTC U0073 or U2100
U0074 | Control Module Communication Bus B Off | -- | DTC U0074
U0100 - U0299 | Lost Communication With XXX Control Module | -- | DTC U0100-U0299
U0301 | Software Incompatibility with Engine Control Module | -- | DTC U0300-U0336
U0315 | Software Incompatibility with Electronic Brake Control Module | -- | DTC U0300-U0336
U0400 - U05FF | Invalid Data Received | -- | DTC U0400-U05FF
U1500 - U15BF | Inter-device Dedicated Bus | -- | DTC U1500-U15BF
U1814 | Powertrain Wake Up Communication Circuit | BCM | DTC U1814
U18B9 - U18BF | Primary High Speed Controller Area Network Bus Subnet Configuration List | -- | DTC U18B9-U18BF
U2100 | Controller Area Network Bus Communication | -- | DTC U0073 or U2100
U2105 - U2199 | Lost Communication With XXX Control Module | -- | DTC U2105-U2199