For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove instrument panel compartment. Refer to Instrument Panel Compartment Replacement.

1 | Mobile Telephone Control Module Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m(44 lb in)
2 | Mobile Telephone Control Module Assembly (2)

#### Procedure

1. Disconnect the mobile telephone control module wiring harness plug.
2. Disconnect the telephone transceiver bracket.