For 1990-2009 cars

## Fastener Tightening Specifications D16

Application | Specification
--- | ---
Metric | English
5th Gear Fork Bolts | 22 N·m | 16 lb ft
5th Gearshift Connector Bolts | 7 N·m | 62 lb in
Backup Lamp Switch | 20 N·m | 15 lb ft
Bearing-Adjusting Ring-Retainer Plate Bolt | 5 N·m | 44 lb in
Bearing Plate Bolts | 22 N·m | 16 lb ft
Bearing Retainer Bolts, Right Side | 25 N·m | 18 lb ft
Clutch and Differential Housing Cover Bolts | 40 N·m | 30 lb ft
Flywheel Inspection Cover Bolts | 7 N·m | 62 lb in
Input Driveshaft Detent Screw | 15 N·m | 11 lb ft
Manual Transmission Selector Shift Lever Cable Bracket Bolt | XX N·m | XX lb ft
Ring-Gear Bolts | 70 N·m | 52 lb ft
Rod Clamp Bolt | 14 N·m | 124 lb in
Speedometer-Driven Gear Bolt | 4 N·m | 35 lb in
Transmission Case Plug | XX N·m | XX lb ft
Transmission Control Bolts | 8 N·m | 71 lb in
Transmission Cover Bolts | 18 N·m | 13 lb ft
Transmission Front Mount Bolts - to Transmission | 100 N·m | 74 lb ft
Transmission Front Mount Bolt - to Front Suspension Frame | 58 N·m | 43 lb ft
Transmission Lower Bolts | 75 N·m | 56 lb ft
Transmission Lower Bolt | 35 N·m | 26 lb ft
Transmission Mount Bracket Bolts - Left Side - to Transmission | 62 N·m | 46 lb ft
Transmission Mount Bolts - Left Side - to Transmission Mount Bracket | 50 N·m + 60-75° | 37 lb ft + 60-75°
Transmission Mount Bolts - Left Side - to Chassis | 62 N·m | 46 lb ft
Transmission Mount Nut - Left Side - to Chassis | 62 N·m | 46 lb ft
Transmission Oil Drain Plug | XX N·m | XX lb ft
Transmission Rear Mount Bolts - to Front Suspension Frame | XX N·m | XX lb ft
Transmission Rear Mount Bracket Bolts - to Transmission | 100 N·m | 74 lb ft
Transmission Rear Mount Bracket Bolt - to Transmission Rear Mount | 100 N·m | 74 lb ft
Transmission Upper Bolts | 75 N·m | 56 lb ft