For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the instrument panel lower trim panel - left side. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side.
2. Remove the instrument panel lower trim panel - right side. Refer to Instrument Panel Lower Trim Panel Replacement - Right Side.
3. Remove the front floor console rear cover. Refer to Front Floor Console Rear Cover Replacement.
4. Remove the front floor console storage tray screw. Refer to Front Floor Console Storage Tray Replacement.
5. Remove the front floor console armrest. Refer to Front Floor Console Armrest Replacement.

1 | Front Floor Console Screw (Qty: 10) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m(X lb in)
2 | Front Floor Console Assembly

#### Procedure

Disconnect the electrical connections.