For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Differential Carrier Baffle Bolts M6 x 25 (Qty: 2)
2 | Front Differential Carrier Baffle
3 | Front Differential Ring Gear Retainer Tip Note the direction of the taper to ensure proper installation.
4 | Front Differential Ring Gear
5 | Fluid Pump Bolts M8 x 33 (Qty: 8)
6 | Fluid Pump Assembly
7 | Torque Converter and Differential Housing Seal