For 1990-2009 cars

Warning: Brake fluid may irritate eyes and skin. In case of contact, take the following actions:

• | Eye contact--rinse thoroughly with water.

• | Skin contact--wash with soap and water.

• | If ingested--consult a physician immediately.

Caution: Brake fluid will damage electrical connections and painted surfaces. Use shop cloths, suitable containers, and fender covers to prevent brake fluid from contacting these areas. Always re-seal and wipe off brake fluid containers to prevent spills.

Caution: Avoid spilling brake fluid on any of the vehicle's painted surfaces, wiring, cables or electrical connectors. Brake fluid will damage paint and electrical connections. If any fluid is spilled on the vehicle, immediately flush the area with water to minimize the potential for damage.

Caution: Power steering fluid, engine oil, brake fluid, or any mineral based fluids cannot be mixed. If brake seals contact power steering fluid or steering seals contact brake fluid, seal damage will result.

Note:

• | Do not reuse the brake fluid collected during the hydraulic brake system bleeding

• | Always store brake fluid in a closed container.

• | Reseal brake fluid containers immediately after use.

• | Do not use brake fluid left in an open container.

• | Do not use brake fluid left in an improperly sealed container.

• | Do not use the following fluids in the hydraulic brake system:

- | Power steering fluid

- | Automatic transmission fluid

- | DOT 5 silicone hydraulic brake fluid

For the correct brake fluid, refer to Adhesives, Fluids, Lubricants, and Sealers.