For 1990-2009 cars

### Removal Procedure

1. Remove instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement.
2. Remove instrument panel wiring harness (2) from instrument panel tie bar (1).

Disconnect electrical connectors.

### Installation Procedure

1. Install instrument panel wiring harness (2) from instrument panel tie bar (1).

Connect electrical connectors.

2. Install instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement.