For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Warning: Refer to Glass and Sheet Metal Handling Warning in the Preface section.

Remove the rear compartment sill trim plate--Refer to Rear Compartment Sill Trim Plate Replacement.

1 | Back Up Lamp Socket Tip Rotate the lamp socket counter clockwise and remove from the tail lamp housing.
2 | Back Up Lamp Bulb Warning: Refer to Halogen Bulb Warning in the Preface section.

#### Procedure

Remove the bulb from the lamp socket.