For 1990-2009 cars

## Rear Wheel Speed Sensor Replacement Disc Brake

### Removal Procedure

1. Remove rear wheelhouse panel liner. Refer to Rear Wheelhouse Panel Liner Replacement.
2. Remove the wheel speed sensor screw (2) from the steering knuckle.
3. Remove wheel speed sensor (1).
4. Remove wiring harness (3) from bracket (4).
5. Disconnect the electrical connector (1).
6. Remove wheel speed sensor from vehicle.

### Installation Procedure

1. Install the wheel speed sensor to the vehicle
2. Connect the electical connector (1).
3. Install the wheel speed sensor (1) to steering knuckle.
4. Install wiring harness (3) at the bracket (4).

Caution: Refer to Fastener Caution in the Preface section.

5. Install the wheel speed sensor screw (2) and tighten to 9 N·m (80 lb in).
6. Install rear wheelhouse panel liner. Refer to Rear Wheelhouse Panel Liner Replacement.

## Rear Wheel Speed Sensor Replacement Drum Brake

### Removal Procedure

1. Remove rear wheelhouse panel liner. Refer to Rear Wheelhouse Panel Liner Replacement.
2. Remove the wheel speed sensor screw (2) from the steering knuckle.
3. Remove wheel speed sensor (1).
4. Remove wiring harness (3) from bracket (4).
5. Disconnect the electrical connector (1).
6. Remove wheel speed sensor from vehicle.

### Installation Procedure

1. Install the wheel speed sensor to the vehicle.
2. Connect the electical connector (1).
3. Install the wheel speed sensor (1) to steering knuckle.
4. Install wiring harness (3) at the bracket (4).

Caution: Refer to Fastener Caution in the Preface section.

5. Install the wheel speed sensor screw (2) and tighten to 9 N·m (80 lb in).
6. Install rear wheelhouse panel liner. Refer to Rear Wheelhouse Panel Liner Replacement.