For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to Brake Fluid Irritant Warning in the Preface section. Caution: Refer to Brake Fluid Effects on Paint and Electrical Components Caution in the Preface section.

#### Preliminary Procedure

Remove and discard the brake fluid from the master cylinder reservoir.

1 | Brake Fluid Level Indicator Switch

#### Procedure

1. Disconnect electrical connector.
2. Rotate indicator switch clockwise to remove.