For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the rear side door stationary window. Refer to Rear Side Door Stationary Window Replacement.
2. Remove the rear side door window frame front cover. Refer to Rear Side Door Window Frame Front Cover Replacement.

1 | Rear Side Door Window Weatherstrip

#### Procedure

Pull the rear side door window weatherstrip away from the outer window flange to remove.