For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Valve Body Ball Check Valve (Qty: 6)
2 | Control Valve Channel Plate Spacer Plate Assembly
3 | Valve Channel Plate Tip Inspect the channel plate bolt pass through holes for damage or burnelling. Any damage could cause leaking. Replace as necessary.
4 | Control Valve Body Bolt M5 x 40.5 (Qty: 1) Caution: Refer to Fastener Caution in the Preface section. Tighten 8 N·m (71 lb in)
5 | Control Solenoid Valve Support