For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to Battery Disconnect Warning in the Preface section.

#### Preliminary Procedure

Remove instrument panel lower trim panel - Right Side. Refer to Instrument Panel Lower Trim Panel Replacement - Right Side.

1 | Body Control Module Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten: 2.5 N·m (23 lb in)
2 | Body Control Module

#### Procedure

1. Disconnect body control module wiring harness plug.
2. Refer to Control Module References for programming and set up procedures.