For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the center pillar lower garnish molding. Refer to LINK.
2. Remove the front seat outer recliner upper finish cover. Refer to LINK.

1 | Center Pillar Upper Garnish Molding Clip
2 | Center Pillar Lower Garnish Molding Assembly

#### Procedure

When replacing the center pillar lower garnish molding, remove the seat belt through the molding.