For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Fluid Pump Seal Assembly
2 | Torque Converter Housing Gasket
3 | Torque Converter (w/Fluid Pump) Housing Assembly Tip Rotate the differential slightly in each direction using DT-47793 rotating tool to align the Differential Pinion Gears with the Differential Ring Gear in the Torque Converter Housing.

#### Special Tool

DT-47793 Differential Rotating Tool

For equivalent regional tools, refer to Special Tools.

4 | Torque Converter and Differential Housing Bolts M8 x 30 (Qty: 15) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Tighten the bolts in sequence shown.

Tighten
10 N·m (89 lb in) then rotate the bolt an additional 50 degrees

#### Special Tool

EN-45059 Angle Meter or equivalent

For equivalent regional tools, refer to Special Tools.