For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear Floor Console Hinge Cover Closeout Screw (Qty: 12) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Rear Floor Console Hinge Cover Closeout Panel
3 | Rear Floor Console Armrest Hinge Screw (Qty: 4) Tighten 2.5 N·m (22 lb in)
4 | Rear Floor Console Armrest Assembly

#### Procedure

When replacing the rear floor console armrest assembly, transfer all necessary components.