For 1990-2009 cars

## Instrument Panel Compartment Trim Plate Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement .

1 | Instrument Panel Compartment Trim Plate Assembly

#### Procedure

1. Disconnect the electrical connections.
2. When replacing the instrument panel compartment trim plate, transfer all necessary components.

2 | Retainer Clip (Qty: 4)

## Instrument Panel Compartment Trim Plate Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement .

1 | Instrument Panel Compartment Trim Plate Assembly

#### Procedure

1. Disconnect the electrical connections.
2. When replacing the instrument panel compartment trim plate, transfer all necessary components.

2 | Retainer Clip (Qty: 4)

## Instrument Panel Compartment Trim Plate Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement.

1 | Instrument Panel Compartment Trim Plate Assembly

#### Procedure

1. Disconnect the electrical connections.
2. When replacing the instrument panel compartment trim plate, transfer all necessary components.

2 | Retainer Clip (Qty: 4)

## Instrument Panel Compartment Trim Plate Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel compartment assembly. Refer to Instrument Panel Compartment Replacement.

1 | Instrument Panel Compartment Trim Plate Assembly

#### Procedure

1. Grasp the compartment trim plate and pull rearward releasing the trim plate from the instrument panel assembly.
2. Disconnect the electrical connections.
3. When replacing the instrument panel compartment trim plate, transfer all necessary components.