For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Door Window Regulator Bolts | 10 N·m | 89 lb in
Door Window Regulator to Door Bolts | 10 N·m | 89 lb in
Door Window Regulator Motor Bolts to Door | 9 N·m | 80 lb in
Door Window Regulator Motor to Regulator Bolts | 5 N·m | 44 lb in
Endgate Molding Retaining Screws | 3 N·m | 27 lb in
Front Door Window Regulator Clamp Nuts | 10 N·m | 89 lb in
Front Door Window Weatherstrip/Run Channel Retaining Bolts | 10 N·m | 89 lb in
Liftgate Window Striker Nuts | 6 N·m | 53 lb in
Side Reveal Molding Screws | 2 N·m | 18 lb in