For 1990-2009 cars

## Rear License Plate Lamp Bulb Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear license plate lamp. Refer to Rear License Lamp Replacement .

1 | Rear License Plate Lamp Bulb Socket (Qty: 2)
2 | Rear License Plate Lamp Bulb (Qty: 2)

#### Procedure

Hold the lamp socket and pull the lamp bulb straight from the lamp socket.

## Rear License Plate Lamp Bulb Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear license plate lamps. Refer to Rear License Lamp Replacement.

1 | Rear License Plate Lamp Bulb (Qty: 2)

#### Procedure

Pull the bulbs straight from the lamp sockets.

## Rear License Plate Lamp Bulb Replacement Acadia

Callout | Component Name
--- | ---
1 | Rear License Plate Lamp Screws (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Rear License Plate Lamp (Qty: 2)

#### Procedure

Pull the lamps downward and disconnect the bulb from the lamp sockets.