For 1990-2009 cars

## Rear Window Washer Nozzle Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the rear wiper arm. Refer to Rear Window Wiper Arm Replacement.
2. Using a pair of locking type pliers, grip the nozzle and pull the nozzle directly out from the wiper arm.
3. Disconnect the rear wiper arm washer hose from the nozzle.

1 | Rear Wiper Arm Nozzle

## Rear Window Washer Nozzle Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear spoiler. Refer to Rear Spoiler Replacement.

1 | Rear Window Washer Nozzle

#### Procedure

1. Squeeze the outer tabs on the nozzle in order to remove the nozzle from the rear spoiler.
2. Disconnect the rear window washer nozzle hose from thew nozzle.
3. Remove the rear window washer nozzle.

## Rear Window Washer Nozzle Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the rear wiper arm blade. Refer to Rear Window Wiper Arm Replacement.
2. Using a pair of locking type pliers, grip the nozzle and pull the nozzle directly out from the wiper arm.
3. Disconnect the rear wiper arm washer hose from the nozzle.

1 | Rear Wiper Arm Nozzle

## Rear Window Washer Nozzle Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear spoiler. Refer to Rear Spoiler Replacement.

1 | Rear Window Washer Nozzle

#### Procedure

1. Squeeze the outer tabs on the nozzle in order to remove the nozzle from the underside of the rear spoiler.
2. Disconnect the rear window washer nozzle hose from the nozzle.
3. Remove the rear window washer nozzle.