For 1990-2009 cars

## Rear Bumper Fascia Reflector Replacement Acadia and OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear bumper fascia reinforcement. Refer to Rear Bumper Fascia Reinforcement Replacement.

1 | Rear Bumper Fascia Reflector Tip Push forward on the tab in order to remove the reflector from the fascia.

## Rear Bumper Fascia Reflector Replacement Enclave and Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise and support the vehicle with suitable safety stands. Refer to Lifting and Jacking the Vehicle.

1 | Rear Bumper Fascia Reflector Bolts (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Rear Bumper Fascia Reflector