For 1990-2009 cars

## Rear Seat Inner Recliner Cable Replacement Short Cable with 40 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat . Refer to Rear Seat Replacement .
2. Remove the rear seat outboard outer recliner cover. Refer to Rear Seat Recliner Outer Finish Cover Replacement - Inboard .
3. Remove the rear back cushion filler panel. Refer to Rear Seat Back Filler Panel Replacement .

1 | Rear Seat Back Latch Release Cable

#### Procedure

1. Note the routing of the cable for installation purposes.
2. Disconnect the cable from the recliner.
3. Note the location of the retainer clip when removing the cable and always make sure the cable is attached to the clip in the same location.

## Rear Seat Inner Recliner Cable Replacement Long Cable with 40 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat . Refer to Rear Seat Replacement .
2. Remove the rear seat outboard outer recliner cover. Refer to Rear Seat Recliner Outer Finish Cover Replacement - Inboard .
3. Remove the rear back cushion filler panel. Refer to Rear Seat Back Filler Panel Replacement .

1 | Rear Seat Inner Recliner Cable

#### Procedure

1. Note the routing of the cable for installation purposes.
2. Disconnect the cable from the recliner.
3. Note the location of the zip tie when removing the cable and always use a new zip tie in the same location when installing the cable.

## Rear Seat Inner Recliner Cable Replacement Short Cable with 60 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat . Refer to Rear Seat Replacement .
2. Remove the rear seat outboard outer recliner cover. Refer to Rear Seat Recliner Outer Finish Cover Replacement - Inboard .
3. Remove the rear back cushion filler panel. Refer to Rear Seat Back Filler Panel Replacement .

1 | Plastic Retainer Clip Tip Note the location of the retainer clip when removing the cable and always make sure the cable is attached to the clip in the same location.
2 | Rear Seat Back Latch Release Cable

#### Procedure

1. Note the routing of the cable for installation purposes.
2. Disconnect the cable from the recliner.

## Rear Seat Inner Recliner Cable Replacement Long Cable with 60 Percent Seat

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear seat . Refer to Rear Seat Replacement .
2. Remove the rear seat outboard outer recliner cover. Refer to Rear Seat Recliner Outer Finish Cover Replacement - Inboard .
3. Remove the rear back cushion filler panel. Refer to Rear Seat Back Filler Panel Replacement .

1 | Retainer Clip Tip Note the location of the retainer clip when removing the cable and always make sure the cable is attached to the clip in the same location.
2 | Rear Seat Back Latch Release Cable

#### Procedure

1. Note the routing of the cable for installation purposes.
2. Disconnect the cable from the recliner.