For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Fuel Filler Door Bolts | 2.5 N·m | 22 lb in
Front Door Check Link Bolts | 10 N·m | 89 lb in
Front Door Check Link to Body | 20 N·m | 15 lb ft
Front Door Hinge To Body Bolts | 36 N·m | 27 lb ft
Front Door Hinge To Door Bolts | 25 N·m | 18 lb ft
Front Fender Bolts | 9 N·m | 80 lb in
Front Outer Door Panel Bolts | 8 N·m | 71 lb in
Hood Hinge Bolts | 25 N·m | 18 lb ft
Hood Latch Bolts | 10 N·m | 89 lb in
Liftgate Hinge Bolts | 25 N·m | 18 lb ft
Liftgate Hinge Nuts | 25 N·m | 18 lb ft
Liftgate Strut Anchor | 25 N·m | 18 lb ft
Quarter Panel Bolts | 9 N·m | 80 lb in
Quarter Panel Nuts | 9 N·m | 80 lb in
Rear Door Check Link Bolts | 10 N·m | 89 lb in
Rear Door Check Link to Body Bolt | 20 N·m | 15 lb ft
Rear Door Hinge To Body Bolts | 36 N·m | 27 lb ft
Rear Door Hinge To Door Bolts | 25 N·m | 18 lb ft
Rear Outer Door Panel Bolts | 8 N·m | 71 lb in
Hood Latch Release Cable Bolt | 9 N·m | 80 lb in
Fuel Tank Filler Door Bolt | 2.5 N·m | 22 lb in
Hood Latch Release Handle Screw | 10 N·m | 89 lb in