For 1990-2009 cars

Checks | Causes
--- | ---
Front Differential Drive Pinion (w/Transfer Gear) Gear Assembly (481) |

• | Inspect for broken or stripped Park Gear splines

• | Inspect for broken or worn Park Gear

Front Differential Carrier Assembly (486) | Inspect for damaged, broken or loose Front Differential Ring Gear
Output Carrier Transfer Drive Gear Hub Assembly (477) |

• | Inspect for worn, stripped or broken splines

• | Inspect for disengaged hub to Transfer Drive Gear

Reaction Carrier Assembly (467) |

• | Inspect for worn, stripped or broken splines

• | Inspect for disengaged to the Output Sun Gear (475)

Case Assembly (507) |

• | Inspect for broken or damaged Case

• | Inspect for loose or stripped Park Pawl Actuator Bracket Bolts (500)

• | Inspect for broken or bent Park Pawl Actuator Bracket (501)

• | Inspect for broken or missing Park Pawl Actuator Guide Pin (505) or Manual Shaft Pin (510)

• | Inspect for broken, loose or misaligned Park Pawl Guide (506)

• | Inspect for binding or broken Park Pawl (503) or Actuator Assembly (509)

Manual Shift Detent Lever Assembly (511) | Inspect for broken or disengaged Manual Valve Link Pin