For 1990-2009 cars

## Side Window Defogger Outlet Grille Replacement - Left Side Enclave

Callout | Component Name
--- | ---
1 | Left Instrument Panel Trim Panel. Refer to Instrument Panel Trim Panel Replacement - Left Side.
2 | Instrument Panel Left Window Air Outlet

#### Procedure

Release the tab on the air outlet from the underside of the trim panel and push the air outlet upward out of the trim panel.

## Side Window Defogger Outlet Grille Replacement - Left Side Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the left instrument panel air outlet assembly. Refer to Instrument Panel Outer Air Outlet Replacement - Left Side.

1 | Pal Nuts (Qty: 3)

#### Procedure

Tighten the pal nuts until fully seated but not stripped

2 | Side Window Defroster Outlet Duct Assembly
3 | Side Window Defroster Outlet Grille Assembly