For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the child seat bracket trim cover. Refer to Rear Seat Number 2 Child Seat Bracket Replacement .
2. Remove the rear seat back cushion release handle bezel. Refer to Rear Seat Pull Strap Replacement .
3. Unzip the side zippers of the rear number 2 back trim cover.
4. Flip the carpet of the back trim over to expose the panel.

1 | Rear Seat No. 2 Back Cushion Panel Tip Using a trim tool or equivalent, pull rearward on the seat back cushion panel to remove.