For 1990-2009 cars

## Rear Side Door Window Switch Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement.

1 | Rear Side Door Window Switch Assembly Tip Use a small flat bladed tool to aid in the removal of the switch from the trim panel.

## Rear Side Door Window Switch Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement.

1 | Rear Side Door Window Switch Assembly Tip Use a small flat bladed tool to aid in the removal of the switch from the trim panel.

## Rear Side Door Window Switch Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove rear door trim panel. Refer to Rear Side Door Trim Panel Replacement.

1 | Rear Switch Plate Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Rear Switch Plate Assembly Tip Use a flat-bladed tool to pry switch plate from door trim.
3 | Rear Side Door Window Switch Assembly Tip Disconnect electrical connectors.

## Rear Side Door Window Switch Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove rear door trim panel. Refer to Rear Side Door Trim Panel Replacement.

1 | Rear Switch Plate Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Rear Switch Plate Assembly Tip Use a flat-bladed tool to pry switch plate from door trim.
3 | Rear Side Door Window Switch Assembly Tip Disconnect electrical connectors.