For 1990-2009 cars

## Instrument Panel Accessory Trim Plate Replacement Acadia

Callout | Component Name
--- | ---
1 | Accessory Trim Plate Assembly

#### Procedure

1. Use a flat-bladed plastic trim tool in order to release the accessory trim plate from the instrument panel assembly.
2. Disconnect the electrical connections.
3. When replacing the accessory trim plate, transfer all necessary components.

2 | Retainer Clip (Qty: 8)

## Instrument Panel Accessory Trim Plate Replacement Enclave

Callout | Component Name
--- | ---
1 | Accessory Trim Plate Assembly

#### Procedures

1. Use a flat bladed plastic trim tool in order to release the accessory trim plate from the instrument panel assembly.
2. Disconnect the electrical connections.
3. When replacing the accessory trim plate, transfer all necessary components.

2 | Retainer Clips (Qty: 8)

## Instrument Panel Accessory Trim Plate Replacement OUTLOOK

Callout | Component Name
--- | ---
1 | Accessory Trim Plate Assembly

#### Procedure

1. Use a flat-bladed plastic trim tool in order to release the accessory trim plate from the instrument panel assembly.
2. Disconnect the electrical connections.
3. When replacing the accessory trim plate, transfer all necessary components.

2 | Retainer Clip (Qty: 8)

## Instrument Panel Accessory Trim Plate Replacement Traverse

Callout | Component Name
--- | ---
1 | Instrument Panel Accessory Trim Plate Assembly

#### Procedures

1. Use a flat bladed plastic trim tool in order to release the clips securing the instrument panel accessory trim plate to the instrument panel assembly.
2. Disconnect the electrical connections.
3. When replacing the accessory trim plate, transfer all necessary components.