For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Tire and Wheel Assembly - Lateral and Radial

- Off-Vehicle

1.27 mm

0.050 in

- On-Vehicle

1.52 mm

0.060 in

Wheel, Aluminum

- Lateral

0.762 mm

0.030 in

- Radial

0.762 mm

0.030 in

Wheel, Steel

- Lateral

1.143 mm

0.045 in

- Radial

1.015 mm

0.040 in

Wheel Hub/Axle Flange - Guideline | 0.132 mm | 0.0052 in
Wheel Stud - Guideline | 0.25 mm | 0.010 in