For 1990-2009 cars

## Rear License Plate Lamp Replacement Enclave

Callout | Component Name
--- | ---
1 | Rear License Plate Lamp Screw (Qty: 4)
2 | Rear License Plate Lamp Housing (Qty: 2)

#### Procedure

Pull the lamp housing downward from the applique and disconnect the bulb socket from the housing by rotating counterclockwise a quarter turn.

## Rear License Plate Lamp Replacement Acadia

Callout | Component Name
--- | ---
1 | Rear License Plate Lamp Screws (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Rear License Plate Lamp (Qty: 2)

#### Procedure

Pull the lamps downward and disconnect the bulb sockets from the lamps.

## Rear License Plate Lamp Replacement OUTLOOK

Callout | Component Name
--- | ---
1 | Rear License Plate Lamp Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Rear License Plate Lamp (Qty: 2)

#### Procedure

Pull the lamps downward and disconnect the bulb sockets from the lamps.