For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Engine Mount to Frame Nut | 75 N·m | 55 lb ft
Frame Brace Bolt | 60 N·m | 44 lb ft
Front Crossmember Brace Bolt | 50 N·m | 37 lb ft
Front Frame to Body Bolt | 110 N·m | 81 lb ft
+ 90 degrees
Front Wheelhouse Liner Screw | 2.5 N·m | 22 lb in
Radiator Support Bolt | 50 N·m | 37 lb ft
Rear Axle Differential to Body Bolt | 160 N·m | 118 lb ft
Rear Brake Caliper Bracket Bolt | 50 N·m | 37 lb ft
Rear Frame Reinforcement Bolt | 60 N·m | 44 lb ft
Rear Frame Reinforcement Stud | 60 N·m | 44 lb ft
Rear Shock Absorber Bolt | 50 N·m | 37 lb ft
Rear Suspension Crossmember to Body Bolt | 170 N·m | 125 lb ft
Rear Wheelhouse Liner Screw | 2.5 N·m | 22 lb in
Right Park Brake Cable Retaining Bolt | 10 N·m | 89 lb in
Trailer Hitch Bolt | 100 N·m | 74 lb ft
Transmission Mount to Frame Nut | 75 N·m | 55 lb ft
Underbody Side Rail Bolt | 47 N·m | 35 lb ft
Underbody Side Rail Nut | 11 N·m | 97 lb in
Upper Bumper Support to Radiator Support Bolt | 9 N·m | 80 lb in
Wheel Drive Shaft Nut | 260 N·m | 192 lb ft