For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Torque Converter Assembly Caution: Lower the torque converter straight down. Failure to lower the torque converter straight down could damage the torque converter clutch lip seal inside the torque converter clutch assembly.

#### Special Tools

J 46409 Torque Converter Lifting Handles

For equivalent regional tools, refer to Special Tools.

2 | J 21366 Converter Holding Strap Warning: The torque converter must be held to the torque converter housing by a retaining device such as shipping brackets. Without the retaining device, the torque converter may slide forward, disengaging the oil pump, or may fall completely out of the transmission causing personal injury and/or property damage.
3 | Dust Cover - Model Dependant
4 | Dust Cover Push Pin - Model Dependant (Qty: 2)
5 | Dust Cover Bolt - Model Dependant Caution: Refer to Fastener Caution in the Preface section. Tighten 75 N·m (37 lb ft)