For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Input Shaft Thrust Bearing Tip Note location of the orientation lip on bearing. All thrust bearings can only be assembled one way.
2 | A/Trans Case Cover Gasket
3 | Input Speed Sensor Wire Harness Tip Route the input speed sensor wire harness through the case passage.
4 | A/Trans Case Cover Assembly

#### Procedure

1. Use guide pins to install the case cover assembly to prevent damage to the input shaft thrust bearing.
2. Pull the input speed sensor wire harness through the case passage while lowering the cover assembly onto the case.

#### Special Tools

39068 Guide Pins

For equivalent regional tools, refer to Special Tools.

5 | A/Trans Case Cover Assembly Bolt M6 x 30 (Qty: 10) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Tighten in sequence shown.

Tighten
12 N·m (9 lb ft)