For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Information Center Telltale Assembly Bezel

#### Procedure

1. Position a flat bladed plastic trim tool between the headliner and the rear of the information center telltale assembly bezel to release the tab retaining the bezel to the headliner.
2. Disconnect the electrical connector.

2 | Parking Aid Monitor Module

#### Procedure

Pull the tabs outwards to release the module from the bezel.