For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Disable the SIR system. Refer to SIR Disabling and Enabling.

1 | Windshield Side Garnish Molding Bolt Hole Finish Plug (Qty: 2)
2 | Windshield Side Garnish Molding Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | Windshield Side Garnish Molding Assembly Tip Disconnect the electrical connector.