For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front floor console accessory trim plate. Refer to Front Floor Console Accessory Trim Plate Replacement.

1 | Front Floor Console Accessory Switch Mounting Plate Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Front Floor Console Accessory Switch Mounting Plate

#### Procedure

Disconnect the electrical connectors.

3 | Seat Heater Switch (Qty: 2)

#### Procedure

Disengage the heated seat switches from the accessory switch mounting plate.