For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Torque Converter Fluid Seal Caution: Support the back side of the torque converter housing while installing the seal. Install the seal until it stops moving. Applying excessive pressure to the seal once it is seated could cause damage to the torque converter housing casting.

#### Special Tools

• | J 6125-1B Slide Hammer with Adapter or equivalent

• | J 23129 Universal Seal Remover

• | J 38693 Seal Installer

For equivalent regional tools, refer to Special Tools.