For 1990-2009 cars

## Liftgate Garnish Molding Replacement withoutTB4

Callout | Component Name
--- | ---
1 | Liftgate Upper Trim Finish Panel Retainer (Qty: 6)
2 | Liftgate Upper Trim Finish Panel Assembly

## Liftgate Garnish Molding Replacement with TB5

Callout | Component Name
--- | ---
1 | Liftgate Actuator Rod
2 | Liftgate Actuator Rod Stud Caution: Refer to Fastener Caution in the Preface section. Tighten 20 N·m (15 lb ft)
3 | Liftgate Upper Trim Finish Panel Assembly