For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the instrument panel trim pad. Refer to Instrument Panel Trim Pad Replacement .
2. Remove the radio. Refer to Radio Replacement .

1 | Navigation Antenna Assembly

#### Procedure

1. Disconnect the navigation antenna from the radio.
2. Pull the tab back to release the navigation antenna from the I/P upper trim pad.
3. Note the location and routing of the gps antenna prior to removing to ensure proper reinstallation.