For 1990-2009 cars

## Rear Seat Cushion Front Cover Replacement with 40 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Cushion Trim Panel Assembly

#### Procedure

Release the tabs and the front and rear of the panel and pull outward to disengage the retainer clips.

2 | Rear Seat Cushion Trim Panel Assembly

#### Procedure

Release the tabs and the front and rear of the panel and pull outward to disengage the retainer clips.

3 | Rear Seat Cushion Front Cover

#### Procedure

Pull forward and use a flat bladed tool to help disengage the retainer clips from the seat cushion frame.