For 1990-2009 cars

## Front Side Door Garnish Molding Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement - Left Side or Front Side Door Trim Panel Replacement - Right Side.

1 | Front Side Door Garnish Molding Retainer Tip Use a door trim panel removal tool or equivalent to aid in the removal of the retainer.
2 | Front Side Door Garnish Molding Tip Pull outward starting at the front and moving slowly rearward to remove the molding.
3 | Front Side Door Garnish Molding Retainer Clip