For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rocker Panel Extension Molding Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Rocker Panel Extension Molding Bolt Tighten 5.0 N·m (44 lb in)
3 | Rocker Panel Extension Molding Assembly Tip Position the top edge of the molding under the front bottom edge of the rear wheelhouse panel prior to installing the screws.