For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C High Pressure Recirculation Switch | 6 N·m | 53 lb in
A/C Line Bracket Nuts and Bolts | 10 N·m | 8 lb ft
A/C Line Mounting Nuts and Bolts | 15 N·m | 11 lb ft
A/C Underbody Line Bracket Nuts | 4 N·m | 35 lb in
Compressor Bracket Mounting Bolts | 60 N·m | 45 lb ft
Compressor Clutch Plate Retaining Bolt | 18 N·m | 13 lb ft
Compressor Mounting Bolts | 25 N·m | 18 lb ft
HVAC Module Case Screws | 1.5 N·m | 13 lb in
HVAC Module Mounting Bolt | 3 N·m | 27 lb in
HVAC Module Mounting Nuts | 10 N·m | 8 lb ft
Instrument Panel (I/P) Duct Mounting Bolts | 3 N·m | 27 lb in
Rear Duct Mounting Screws | 10 N·m | 8 lb ft