For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Torque Converter - Front Wheel Drive Shaft Oil Seal Assembly Tip Use the open side of J 46629-A seal installer to avoid seal lip damage and to install the seal to the proper depth.

#### Special Tools

• | J 6125-1B Slide Hammer with Adapter

• | J 8092 Driver Handle

• | J 23129 Universal Seal Remover

• | J 46629-A Seal Installer

For equivalent regional tools, refer to Special Tools.