For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Clutch Control Module to Torque Tube Screws | 8 N·m | 71 lb in
Differential-to-Cradle Mount Bolts/Nuts | 28 N·m | 21 lb ft
Differential Rear Mounting bolts | 160 N·m | 118 lb ft
Differential Side Cover Bolts | 28 N·m | 21 lb ft
Lubricant Drain Plug | 35 N·m | 26 lb ft
Lubricant Fill Plug | 35 N·m | 26 lb ft
Pinion Housing-to-Differential Bolts | 28 N·m | 21 lb ft
Torque Tube Bracket-to-Body Bolts | 185 N·m | 137 lb ft
Torque Tube-to-Differential Bolts | 55 N·m | 40 lb ft